(export (version D)
  (design
    (source /home/gaizi/pcb/hisolator/hisolator/hisolator.sch)
    (date "Sun 17 May 2020 11:55:02 AM CST")
    (tool "Eeschema 5.1.5-2.fc32")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source hisolator.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name "/Host Side/") (tstamps /5E73BE76/)
      (title_block
        (title "Hisolator Host Side")
        (company)
        (rev 0.01)
        (date 2020-03-18)
        (source host.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name "/Device Side/") (tstamps /5EDD0BB0/)
      (title_block
        (title "Hisolator Device Side")
        (company)
        (rev 0.01)
        (date 2020-03-18)
        (source device.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U4)
      (value CH317Q)
      (footprint Package_QFP:LQFP-44_10x10mm_P0.8mm)
      (libsource (lib hisolator) (part CH317Q) (description "USB 2.0 Over Ethernet Extension Controller, Low/Full/High Speed USB, RGMII Interface, QFP-44"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC34))
    (comp (ref R4)
      (value 0R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E74124B))
    (comp (ref R5)
      (value 0R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E741252))
    (comp (ref R7)
      (value 2k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E741262))
    (comp (ref R6)
      (value 33R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC38))
    (comp (ref C3)
      (value 20pF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E741279))
    (comp (ref C4)
      (value 20pF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E741280))
    (comp (ref Y1)
      (value 30MHz)
      (footprint Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm)
      (datasheet ~)
      (libsource (lib Device) (part Crystal) (description "Two pin crystal"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E741287))
    (comp (ref C20)
      (value 20pF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC3C))
    (comp (ref C21)
      (value 20pF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E7412A8))
    (comp (ref Y2)
      (value 25MHz)
      (footprint Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm)
      (datasheet ~)
      (libsource (lib Device) (part Crystal) (description "Two pin crystal"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E7412AF))
    (comp (ref R1)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E7412C7))
    (comp (ref R2)
      (value 12k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC41))
    (comp (ref TR1)
      (value SM51589PEL)
      (footprint hisolator:Transformer_Ethernet_Bourns_SM51589PEL)
      (datasheet https://www.haloelectronics.com/pdf/discrete-genesus.pdf)
      (libsource (lib hisolator) (part SM51589PEL) (description "Single Port Gigabit Ethernet Transformers"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E7412EB))
    (comp (ref U1)
      (value LM1117-3.3)
      (footprint Package_TO_SOT_THT:TO-220-3_Vertical)
      (datasheet http://www.ti.com/lit/ds/symlink/lm1117.pdf)
      (libsource (lib Regulator_Linear) (part LM1117-3.3) (description "800mA Low-Dropout Linear Regulator, 3.3V fixed output, TO-220/TO-252/TO-263/SOT-223"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC42))
    (comp (ref C9)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Material) Ceramic))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC43))
    (comp (ref C12)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Material) Ceramic))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC44))
    (comp (ref C23)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E741331))
    (comp (ref R15)
      (value 2.49k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Tolerance) 1%))
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC45))
    (comp (ref R9)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC4D))
    (comp (ref C19)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC4E))
    (comp (ref D1)
      (value LED)
      (footprint LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E8C35E3))
    (comp (ref R13)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E8E7F60))
    (comp (ref R12)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E955762))
    (comp (ref R11)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E955909))
    (comp (ref R10)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC5B))
    (comp (ref D2)
      (value LED)
      (footprint LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC5C))
    (comp (ref R14)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5EA770D0))
    (comp (ref C22)
      (value 1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Material) Ceramic))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5EBA9265))
    (comp (ref C24)
      (value 1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Material) Ceramic))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5EBA926C))
    (comp (ref U5)
      (value RTL8211F)
      (footprint Package_DFN_QFN:QFN-40-1EP_5x5mm_P0.4mm_EP3.6x3.6mm)
      (datasheet https://datasheet.lcsc.com/szlcsc/1909021205_Realtek-Semicon-RTL8211F-CG_C187932.pdf)
      (libsource (lib hisolator) (part RTL8211F) (description "Realtek Integrated 10/100/1000M Ethernet Precision Transceiver, RGMII Interfaces, QFN-40"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E741239))
    (comp (ref U3)
      (value TLV73310PDBVR)
      (footprint Package_TO_SOT_SMD:SOT-23-5)
      (datasheet http://www.ti.com/lit/ds/symlink/tlv713p.pdf)
      (libsource (lib Regulator_Linear) (part TLV71310PDBV) (description "150mA Low Dropout Voltage Regulator, Fixed Output 1.0V, SOT-23-5"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5ED7CF06))
    (comp (ref R3)
      (value 0.1)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5EDA16F6))
    (comp (ref U2)
      (value LM1117-1.8)
      (footprint Package_TO_SOT_THT:TO-220-3_Vertical)
      (datasheet http://www.ti.com/lit/ds/symlink/lm1117.pdf)
      (libsource (lib Regulator_Linear) (part LM1117-3.3) (description "800mA Low-Dropout Linear Regulator, 3.3V fixed output, TO-220/TO-252/TO-263/SOT-223"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5EE17B45))
    (comp (ref C16)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Material) Ceramic))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC67))
    (comp (ref C18)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Material) Ceramic))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5EE17B53))
    (comp (ref R8)
      (value 0.1)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5EE17B6C))
    (comp (ref J1)
      (value Jack-DC)
      (footprint Connector_BarrelJack:BarrelJack_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Jack-DC) (description "DC Barrel Jack"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5EE5579D))
    (comp (ref C1)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC6D))
    (comp (ref C2)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC6E))
    (comp (ref C5)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC6F))
    (comp (ref C6)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC70))
    (comp (ref C7)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC71))
    (comp (ref C8)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC72))
    (comp (ref C10)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC73))
    (comp (ref C11)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC74))
    (comp (ref C13)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F10D7C8))
    (comp (ref C14)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F121E19))
    (comp (ref C15)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F121E20))
    (comp (ref C17)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC79))
    (comp (ref R16)
      (value 0)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F3C6ED8))
    (comp (ref R18)
      (value 0)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC84))
    (comp (ref R19)
      (value 0)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC85))
    (comp (ref R21)
      (value 0)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F505A56))
    (comp (ref R22)
      (value 0)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F541ABB))
    (comp (ref L2)
      (value L_Core_Ferrite)
      (footprint Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part L_Core_Ferrite) (description "Inductor with ferrite core"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F5BDDCC))
    (comp (ref R20)
      (value 0)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F60F840))
    (comp (ref L4)
      (value L_Core_Ferrite)
      (footprint Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part L_Core_Ferrite) (description "Inductor with ferrite core"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F60F847))
    (comp (ref L3)
      (value L_Core_Ferrite)
      (footprint Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part L_Core_Ferrite) (description "Inductor with ferrite core"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC8D))
    (comp (ref L5)
      (value L_Core_Ferrite)
      (footprint Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part L_Core_Ferrite) (description "Inductor with ferrite core"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC8E))
    (comp (ref L6)
      (value L_Core_Ferrite)
      (footprint Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part L_Core_Ferrite) (description "Inductor with ferrite core"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC8F))
    (comp (ref J2)
      (value USB_B_Micro)
      (footprint hisolator:USB_Micro-B_MK5P)
      (datasheet ~)
      (libsource (lib Connector) (part USB_B_Micro) (description "USB Micro Type B connector"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC90))
    (comp (ref C26)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC48))
    (comp (ref C28)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC49))
    (comp (ref C30)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E7A8FCD))
    (comp (ref C25)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC4F))
    (comp (ref C27)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E7C2293))
    (comp (ref C29)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E7DC98C))
    (comp (ref C32)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC54))
    (comp (ref R24)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5E791C40))
    (comp (ref R23)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC52))
    (comp (ref R25)
      (value 33R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F11A93A))
    (comp (ref C64)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F8F0370))
    (comp (ref L1)
      (value L_Core_Ferrite)
      (footprint Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part L_Core_Ferrite) (description "Inductor with ferrite core"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F559B06))
    (comp (ref R17)
      (value 0)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5F2EAC83))
    (comp (ref R51)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5FA62306))
    (comp (ref R50)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5FB8D443))
    (comp (ref U12)
      (value USBLC6-2SC6)
      (footprint Package_TO_SOT_SMD:SOT-23-6)
      (datasheet http://www2.st.com/resource/en/datasheet/CD00050750.pdf)
      (libsource (lib Power_Protection) (part USBLC6-2SC6) (description "Bidirectional ESD Protection Diode, SOT-23-6"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 5FF5C9F3))
    (comp (ref R54)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Host Side/") (tstamps /5E73BE76/))
      (tstamp 60A82C60))
    (comp (ref R37)
      (value 2k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC37))
    (comp (ref C34)
      (value 20pF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5E7412A1))
    (comp (ref C35)
      (value 20pF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC3D))
    (comp (ref Y3)
      (value 25MHz)
      (footprint Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm)
      (datasheet ~)
      (libsource (lib Device) (part Crystal) (description "Two pin crystal"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC3E))
    (comp (ref R27)
      (value 2.49k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Tolerance) 1%))
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5E741376))
    (comp (ref R35)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5E7AECC9))
    (comp (ref C36)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5E7AEDEA))
    (comp (ref D4)
      (value LED)
      (footprint LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC55))
    (comp (ref R29)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC56))
    (comp (ref R32)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC57))
    (comp (ref R31)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC58))
    (comp (ref R30)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5E96AC05))
    (comp (ref D3)
      (value LED)
      (footprint LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5EA770C9))
    (comp (ref R28)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC5D))
    (comp (ref U7)
      (value RTL8211F)
      (footprint Package_DFN_QFN:QFN-40-1EP_5x5mm_P0.4mm_EP3.6x3.6mm)
      (datasheet https://datasheet.lcsc.com/szlcsc/1909021205_Realtek-Semicon-RTL8211F-CG_C187932.pdf)
      (libsource (lib hisolator) (part RTL8211F) (description "Realtek Integrated 10/100/1000M Ethernet Precision Transceiver, RGMII Interfaces, QFN-40"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC35))
    (comp (ref R39)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC4B))
    (comp (ref R41)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5E7CA179))
    (comp (ref U10)
      (value CH317Q)
      (footprint Package_QFP:LQFP-44_10x10mm_P0.8mm)
      (libsource (lib hisolator) (part CH317Q) (description "USB 2.0 Over Ethernet Extension Controller, Low/Full/High Speed USB, RGMII Interface, QFP-44"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5E741232))
    (comp (ref C60)
      (value 20pF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC39))
    (comp (ref C61)
      (value 20pF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC3A))
    (comp (ref Y4)
      (value 30MHz)
      (footprint Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm)
      (datasheet ~)
      (libsource (lib Device) (part Crystal) (description "Two pin crystal"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC3B))
    (comp (ref R46)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC3F))
    (comp (ref R47)
      (value 12k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5E7412DD))
    (comp (ref R42)
      (value 33R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5E74126D))
    (comp (ref R43)
      (value 33R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC76))
    (comp (ref L12)
      (value L_Core_Ferrite)
      (footprint Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part L_Core_Ferrite) (description "Inductor with ferrite core"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F7859B9))
    (comp (ref L10)
      (value L_Core_Ferrite)
      (footprint Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part L_Core_Ferrite) (description "Inductor with ferrite core"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC8B))
    (comp (ref R40)
      (value 0)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC8A))
    (comp (ref L8)
      (value L_Core_Ferrite)
      (footprint Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part L_Core_Ferrite) (description "Inductor with ferrite core"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC89))
    (comp (ref R45)
      (value 0)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC87))
    (comp (ref R44)
      (value 0)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC86))
    (comp (ref R36)
      (value 0)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F48DD97))
    (comp (ref R34)
      (value 0)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F48D99A))
    (comp (ref R26)
      (value 0)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F43F316))
    (comp (ref R38)
      (value 0.1)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC69))
    (comp (ref C45)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Material) Ceramic))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC68))
    (comp (ref C42)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Material) Ceramic))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5EE17B4C))
    (comp (ref U8)
      (value LM1117-1.8)
      (footprint Package_TO_SOT_THT:TO-220-3_Vertical)
      (datasheet http://www.ti.com/lit/ds/symlink/lm1117.pdf)
      (libsource (lib Regulator_Linear) (part LM1117-3.3) (description "800mA Low-Dropout Linear Regulator, 3.3V fixed output, TO-220/TO-252/TO-263/SOT-223"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC66))
    (comp (ref R33)
      (value 0.1)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC65))
    (comp (ref U11)
      (value TLV73310PDBVR)
      (footprint Package_TO_SOT_SMD:SOT-23-5)
      (datasheet http://www.ti.com/lit/ds/symlink/tlv713p.pdf)
      (libsource (lib Regulator_Linear) (part TLV71310PDBV) (description "150mA Low Dropout Voltage Regulator, Fixed Output 1.0V, SOT-23-5"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC64))
    (comp (ref C57)
      (value 1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Material) Ceramic))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC62))
    (comp (ref C52)
      (value 1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Material) Ceramic))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC61))
    (comp (ref C33)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Material) Ceramic))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5E741311))
    (comp (ref C31)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Material) Ceramic))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5E74130A))
    (comp (ref U6)
      (value LM1117-3.3)
      (footprint Package_TO_SOT_THT:TO-220-3_Vertical)
      (datasheet http://www.ti.com/lit/ds/symlink/lm1117.pdf)
      (libsource (lib Regulator_Linear) (part LM1117-3.3) (description "800mA Low-Dropout Linear Regulator, 3.3V fixed output, TO-220/TO-252/TO-263/SOT-223"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5E741303))
    (comp (ref U9)
      (value CH9317G)
      (footprint Package_SO:SOIC-16_3.9x9.9mm_P1.27mm)
      (libsource (lib hisolator) (part CH9317G) (description "PHY Monitoring and Configuration Chip for CH317Q, SOIC-16"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5EE53796))
    (comp (ref R49)
      (value 0)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC82))
    (comp (ref C37)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5E89C012))
    (comp (ref C39)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F121E37))
    (comp (ref C41)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC78))
    (comp (ref C44)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC77))
    (comp (ref C38)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC75))
    (comp (ref C40)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F10D7B1))
    (comp (ref C43)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F10D7AA))
    (comp (ref R48)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F0BF64A))
    (comp (ref C46)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC53))
    (comp (ref C48)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC50))
    (comp (ref C50)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5E7C2288))
    (comp (ref C47)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC4C))
    (comp (ref C49)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5E790E6B))
    (comp (ref C51)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5E790E60))
    (comp (ref C54)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F0EC362))
    (comp (ref C56)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F0EC34B))
    (comp (ref C59)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F0EC344))
    (comp (ref C53)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F087F5E))
    (comp (ref C55)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F036D03))
    (comp (ref C58)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F02A192))
    (comp (ref TP1)
      (value TestPoint)
      (footprint TestPoint:TestPoint_Pad_2.0x2.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint) (description "test point"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F29B3AE))
    (comp (ref C63)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F667888))
    (comp (ref C62)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F667D45))
    (comp (ref J4)
      (value Jack-DC)
      (footprint Connector_BarrelJack:BarrelJack_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Jack-DC) (description "DC Barrel Jack"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5EC648DF))
    (comp (ref L11)
      (value L_Core_Ferrite)
      (footprint Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part L_Core_Ferrite) (description "Inductor with ferrite core"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F73210E))
    (comp (ref L9)
      (value L_Core_Ferrite)
      (footprint Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part L_Core_Ferrite) (description "Inductor with ferrite core"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F639AA2))
    (comp (ref L7)
      (value L_Core_Ferrite)
      (footprint Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part L_Core_Ferrite) (description "Inductor with ferrite core"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F2EAC88))
    (comp (ref J3)
      (value USB_A)
      (footprint Connector_USB:USB_A_Stewart_SS-52100-001_Horizontal)
      (datasheet " ~")
      (libsource (lib Connector) (part USB_A) (description "USB Type A connector"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5ECA8C0B))
    (comp (ref R52)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F48C0EA))
    (comp (ref R53)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 5F76772C))
    (comp (ref U13)
      (value USBLC6-2SC6)
      (footprint Package_TO_SOT_SMD:SOT-23-6)
      (datasheet http://www2.st.com/resource/en/datasheet/CD00050750.pdf)
      (libsource (lib Power_Protection) (part USBLC6-2SC6) (description "Bidirectional ESD Protection Diode, SOT-23-6"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 6018FDA4))
    (comp (ref R55)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 60AEECB4))
    (comp (ref R56)
      (value 2k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/Device Side/") (tstamps /5EDD0BB0/))
      (tstamp 60B78478)))
  (libparts
    (libpart (lib Connector) (part Barrel_Jack)
      (aliases
        (alias Jack-DC))
      (description "DC Barrel Jack")
      (docs ~)
      (footprints
        (fp BarrelJack*))
      (fields
        (field (name Reference) J)
        (field (name Value) Barrel_Jack))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Connector) (part TestPoint)
      (description "test point")
      (docs ~)
      (footprints
        (fp Pin*)
        (fp Test*))
      (fields
        (field (name Reference) TP)
        (field (name Value) TestPoint))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib Connector) (part USB_A)
      (description "USB Type A connector")
      (docs " ~")
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_A))
      (pins
        (pin (num 1) (name VBUS) (type power_in))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name Shield) (type passive))))
    (libpart (lib Connector) (part USB_B_Micro)
      (aliases
        (alias USB_B_Mini))
      (description "USB Micro Type B connector")
      (docs ~)
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_B_Micro))
      (pins
        (pin (num 1) (name VBUS) (type power_out))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name ID) (type passive))
        (pin (num 5) (name GND) (type power_out))
        (pin (num 6) (name Shield) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part C_Small)
      (description "Unpolarized capacitor, small symbol")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Crystal)
      (description "Two pin crystal")
      (docs ~)
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part LED)
      (description "Light emitting diode")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part L_Core_Ferrite)
      (description "Inductor with ferrite core")
      (docs ~)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L_Core_Ferrite))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part R_US)
      (description "Resistor, US symbol")
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R_US))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Power_Protection) (part USBLC6-2SC6)
      (description "Bidirectional ESD Protection Diode, SOT-23-6")
      (docs http://www2.st.com/resource/en/datasheet/CD00050750.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) U)
        (field (name Value) USBLC6-2SC6)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23-6))
      (pins
        (pin (num 1) (name IO1) (type passive))
        (pin (num 2) (name GND) (type passive))
        (pin (num 3) (name IO2) (type passive))
        (pin (num 4) (name IO2) (type passive))
        (pin (num 5) (name VBUS) (type passive))
        (pin (num 6) (name IO1) (type passive))))
    (libpart (lib Regulator_Linear) (part LM1117-1.8)
      (aliases
        (alias LM1117-2.5)
        (alias LM1117-3.3)
        (alias LM1117-5.0)
        (alias TLV1117-15)
        (alias TLV1117-18)
        (alias TLV1117-25)
        (alias TLV1117-33)
        (alias TLV1117-50))
      (description "800mA Low-Dropout Linear Regulator, 1.8V fixed output, TO-220/TO-252/TO-263/SOT-223")
      (docs http://www.ti.com/lit/ds/symlink/lm1117.pdf)
      (footprints
        (fp SOT?223*)
        (fp TO?263*)
        (fp TO?252*)
        (fp TO?220*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM1117-1.8))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))))
    (libpart (lib Regulator_Linear) (part TLV70012_SOT23-5)
      (aliases
        (alias TLV70013_SOT23-5)
        (alias TLV70015_SOT23-5)
        (alias TLV70018_SOT23-5)
        (alias TLV70019_SOT23-5)
        (alias TLV70025_SOT23-5)
        (alias TLV70030_SOT23-5)
        (alias TLV70032_SOT23-5)
        (alias TLV70033_SOT23-5)
        (alias TLV70036_SOT23-5)
        (alias TLV70212_SOT23-5)
        (alias TLV70215_SOT23-5)
        (alias TLV70218_SOT23-5)
        (alias TLV70225_SOT23-5)
        (alias TLV70228_SOT23-5)
        (alias TLV70230_SOT23-5)
        (alias TLV70231_SOT23-5)
        (alias TLV70233_SOT23-5)
        (alias TLV70235_SOT23-5)
        (alias TLV70237_SOT23-5)
        (alias TLV70245_SOT23-5)
        (alias TLV71209_SOT23-5)
        (alias TLV71210_SOT23-5)
        (alias TLV71211_SOT23-5)
        (alias TLV71310PDBV)
        (alias TLV71311PDBV)
        (alias TLV71312PDBV)
        (alias TLV71315PDBV)
        (alias TLV71318PDBV)
        (alias TLV713185PDBV)
        (alias TLV71325PDBV)
        (alias TLV71328PDBV)
        (alias TLV713285PDBV)
        (alias TLV71330PDBV)
        (alias TLV71333PDBV)
        (alias TLV75509PDBV)
        (alias TLV75510PDBV)
        (alias TLV75512PDBV)
        (alias TLV75515PDBV)
        (alias TLV75518PDBV)
        (alias TLV75519PDBV)
        (alias TLV75525PDBV)
        (alias TLV75528PDBV)
        (alias TLV75529PDBV)
        (alias TLV75530PDBV)
        (alias TLV75533PDBV)
        (alias TLV75709PDBV)
        (alias TLV75710PDBV)
        (alias TLV75712PDBV)
        (alias TLV75715PDBV)
        (alias TLV75718PDBV)
        (alias TLV75719PDBV)
        (alias TLV75725PDBV)
        (alias TLV75728PDBV)
        (alias TLV75729PDBV)
        (alias TLV75730PDBV)
        (alias TLV75733PDBV)
        (alias TLV702475_SOT23-5))
      (description "200mA Low Dropout Voltage Regulator, Fixed Output 1.2V, SOT-23-5")
      (docs http://www.ti.com/lit/ds/symlink/tlv700.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) U)
        (field (name Value) TLV70012_SOT23-5)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23-5))
      (pins
        (pin (num 1) (name IN) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name EN) (type input))
        (pin (num 4) (name NC) (type NotConnected))
        (pin (num 5) (name OUT) (type power_out))))
    (libpart (lib hisolator) (part CH317Q)
      (description "USB 2.0 Over Ethernet Extension Controller, Low/Full/High Speed USB, RGMII Interface, QFP-44")
      (footprints
        (fp LQFP?44*10x10mm*P0.8mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) CH317Q))
      (pins
        (pin (num 1) (name VCC18) (type power_in))
        (pin (num 2) (name XI) (type input))
        (pin (num 3) (name XO) (type output))
        (pin (num 4) (name VCC33U) (type power_in))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name RES) (type input))
        (pin (num 7) (name UD-) (type BiDi))
        (pin (num 8) (name UD+) (type BiDi))
        (pin (num 9) (name VCC33U) (type power_in))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name VCC18) (type power_in))
        (pin (num 12) (name VCC18) (type power_in))
        (pin (num 13) (name GND) (type power_in))
        (pin (num 14) (name RXD0) (type input))
        (pin (num 15) (name RXD1) (type input))
        (pin (num 16) (name RXD2) (type input))
        (pin (num 17) (name RXD3) (type input))
        (pin (num 18) (name RXDV) (type input))
        (pin (num 19) (name VCC18) (type power_in))
        (pin (num 20) (name GND) (type power_in))
        (pin (num 21) (name RXCK) (type input))
        (pin (num 22) (name VCC33) (type power_in))
        (pin (num 25) (name GND) (type power_in))
        (pin (num 27) (name TXCK) (type output))
        (pin (num 28) (name TXEN) (type output))
        (pin (num 29) (name VCC18) (type power_in))
        (pin (num 30) (name GND) (type power_in))
        (pin (num 31) (name VCC33) (type power_in))
        (pin (num 32) (name TXD3) (type output))
        (pin (num 33) (name TXD2) (type output))
        (pin (num 34) (name TXD1) (type output))
        (pin (num 35) (name TXD0) (type output))
        (pin (num 36) (name MDC) (type output))
        (pin (num 37) (name MDIO) (type BiDi))
        (pin (num 38) (name MOD0) (type input))
        (pin (num 39) (name VCC18) (type power_in))
        (pin (num 40) (name GND) (type power_in))
        (pin (num 41) (name VCC33) (type power_in))
        (pin (num 42) (name MOD2) (type input))
        (pin (num 43) (name VCC33) (type power_in))
        (pin (num 44) (name GND) (type power_in))))
    (libpart (lib hisolator) (part CH9317G)
      (description "PHY Monitoring and Configuration Chip for CH317Q, SOIC-16")
      (footprints
        (fp SOIC*7.5x10.3mm*P1.27mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) CH9317G)
        (field (name Footprint) Package_SO:SOIC-16_3.9x9.9mm_P1.27mm))
      (pins
        (pin (num 1) (name ~RESET) (type input))
        (pin (num 2) (name PA0) (type BiDi))
        (pin (num 3) (name PA1) (type input))
        (pin (num 4) (name PA2) (type output))
        (pin (num 5) (name VCC) (type power_in))
        (pin (num 6) (name UD+) (type BiDi))
        (pin (num 7) (name UD-) (type BiDi))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name XI) (type input))
        (pin (num 10) (name XO) (type output))
        (pin (num 11) (name PB3) (type BiDi))
        (pin (num 12) (name PB5) (type BiDi))
        (pin (num 13) (name PB6) (type input))
        (pin (num 14) (name PB7) (type output))
        (pin (num 15) (name VCC) (type power_in))
        (pin (num 16) (name PB4) (type BiDi))))
    (libpart (lib hisolator) (part RTL8211F)
      (description "Realtek Integrated 10/100/1000M Ethernet Precision Transceiver, RGMII Interfaces, QFN-40")
      (docs https://datasheet.lcsc.com/szlcsc/1909021205_Realtek-Semicon-RTL8211F-CG_C187932.pdf)
      (footprints
        (fp QFN?40*1EP*5x5mm*P0.4mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) RTL8211F)
        (field (name Footprint) Package_DFN_QFN:QFN-40-1EP_5x5mm_P0.4mm_EP3.6x3.6mm)
        (field (name Datasheet) https://datasheet.lcsc.com/szlcsc/1909021205_Realtek-Semicon-RTL8211F-CG_C187932.pdf))
      (pins
        (pin (num 1) (name MDI0+) (type BiDi))
        (pin (num 2) (name MDI0-) (type BiDi))
        (pin (num 3) (name AVDD10) (type power_in))
        (pin (num 4) (name MDI1+) (type BiDi))
        (pin (num 5) (name MDI1-) (type BiDi))
        (pin (num 6) (name MDI2+) (type BiDi))
        (pin (num 7) (name MDI2-) (type BiDi))
        (pin (num 8) (name AVDD10) (type power_in))
        (pin (num 9) (name MDI3+) (type BiDi))
        (pin (num 10) (name MDI3-) (type BiDi))
        (pin (num 11) (name AVDD33) (type power_in))
        (pin (num 12) (name PHYRSTB) (type input))
        (pin (num 13) (name MDC) (type input))
        (pin (num 14) (name MDIO) (type BiDi))
        (pin (num 15) (name TXD3) (type input))
        (pin (num 16) (name TXD2) (type input))
        (pin (num 17) (name TXD1) (type input))
        (pin (num 18) (name TXD0) (type input))
        (pin (num 19) (name TXCTL) (type input))
        (pin (num 20) (name TXC) (type input))
        (pin (num 21) (name DVDD10) (type power_in))
        (pin (num 22) (name RXD3/PHYAD0) (type BiDi))
        (pin (num 23) (name RXD2/PLLOFF) (type BiDi))
        (pin (num 24) (name RXD1/TXDLY) (type BiDi))
        (pin (num 25) (name RXD0/RXDLY) (type BiDi))
        (pin (num 26) (name RXCTL/PHYAD2) (type BiDi))
        (pin (num 27) (name RXC/PHYAD1) (type BiDi))
        (pin (num 28) (name DVDD_RG) (type power_in))
        (pin (num 29) (name DVDD33) (type power_in))
        (pin (num 30) (name REG_OUT/LDO_OUT) (type output))
        (pin (num 31) (name INTB/PMEB) (type output))
        (pin (num 32) (name LED0/CFG_EXT) (type BiDi))
        (pin (num 33) (name LED1/LDO0) (type BiDi))
        (pin (num 34) (name LED2/LDO1) (type BiDi))
        (pin (num 35) (name CLK_OUT) (type output))
        (pin (num 36) (name XTAL_IN) (type input))
        (pin (num 37) (name XTAL_OUT/EXT_CLK) (type output))
        (pin (num 38) (name AVDD10) (type power_in))
        (pin (num 39) (name RSET) (type output))
        (pin (num 40) (name AVDD33) (type power_in))
        (pin (num 41) (name GND) (type power_in))))
    (libpart (lib hisolator) (part SM51589PEL)
      (description "Single Port Gigabit Ethernet Transformers")
      (docs https://www.haloelectronics.com/pdf/discrete-genesus.pdf)
      (footprints
        (fp Transformer*Ethernet*HALO*TG111*))
      (fields
        (field (name Reference) TR)
        (field (name Value) SM51589PEL)
        (field (name Footprint) Transformer_SMD:Transformer_Ethernet_HALO_TG111-MSC13))
      (pins
        (pin (num 1) (name MCT1) (type passive))
        (pin (num 2) (name MX1+) (type passive))
        (pin (num 3) (name MX1-) (type passive))
        (pin (num 4) (name MCT2) (type passive))
        (pin (num 5) (name MX2+) (type passive))
        (pin (num 6) (name MX2-) (type passive))
        (pin (num 7) (name MCT3) (type passive))
        (pin (num 8) (name MX3+) (type passive))
        (pin (num 9) (name MX3-) (type passive))
        (pin (num 10) (name MCT4) (type passive))
        (pin (num 11) (name MX4+) (type passive))
        (pin (num 12) (name MX4-) (type passive))
        (pin (num 13) (name TD4-) (type passive))
        (pin (num 14) (name TD4+) (type passive))
        (pin (num 15) (name TCT4) (type passive))
        (pin (num 16) (name TD3-) (type passive))
        (pin (num 17) (name TD3+) (type passive))
        (pin (num 18) (name TCT3) (type passive))
        (pin (num 19) (name TD2-) (type passive))
        (pin (num 20) (name TD2+) (type passive))
        (pin (num 21) (name TCT2) (type passive))
        (pin (num 22) (name TD1-) (type passive))
        (pin (num 23) (name TD1+) (type passive))
        (pin (num 24) (name TCT1) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri /usr/share/kicad/library/Connector.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical Power_Protection)
      (uri /usr/share/kicad/library/Power_Protection.lib))
    (library (logical Regulator_Linear)
      (uri /usr/share/kicad/library/Regulator_Linear.lib))
    (library (logical hisolator)
      (uri /home/gaizi/pcb/hisolator/hisolator/lib/hisolator.lib)))
  (nets
    (net (code 1) (name "Net-(L2-Pad1)")
      (node (ref L2) (pin 1))
      (node (ref R18) (pin 1)))
    (net (code 2) (name "Net-(L4-Pad1)")
      (node (ref R20) (pin 1))
      (node (ref L4) (pin 1)))
    (net (code 3) (name +1.8V)
      (node (ref C28) (pin 1))
      (node (ref C30) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref C26) (pin 1))
      (node (ref U4) (pin 11))
      (node (ref U4) (pin 19))
      (node (ref L5) (pin 1))
      (node (ref U4) (pin 29))
      (node (ref U4) (pin 39))
      (node (ref U4) (pin 12))
      (node (ref U4) (pin 1))
      (node (ref L4) (pin 2)))
    (net (code 4) (name "Net-(L6-Pad1)")
      (node (ref L6) (pin 1))
      (node (ref R22) (pin 1)))
    (net (code 5) (name "Net-(J2-Pad1)")
      (node (ref J2) (pin 1)))
    (net (code 6) (name GND)
      (node (ref C21) (pin 2))
      (node (ref C32) (pin 2))
      (node (ref C20) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref C19) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref U2) (pin 1))
      (node (ref C15) (pin 2))
      (node (ref U4) (pin 5))
      (node (ref R2) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref U4) (pin 44))
      (node (ref C22) (pin 2))
      (node (ref U4) (pin 10))
      (node (ref U4) (pin 13))
      (node (ref U4) (pin 20))
      (node (ref R50) (pin 2))
      (node (ref U12) (pin 2))
      (node (ref U4) (pin 25))
      (node (ref C29) (pin 2))
      (node (ref R13) (pin 1))
      (node (ref C24) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref J1) (pin 2))
      (node (ref U4) (pin 30))
      (node (ref U4) (pin 40))
      (node (ref J2) (pin 5))
      (node (ref C25) (pin 2))
      (node (ref C27) (pin 2))
      (node (ref C30) (pin 2))
      (node (ref U5) (pin 41))
      (node (ref U3) (pin 2))
      (node (ref R12) (pin 1))
      (node (ref R11) (pin 1))
      (node (ref R16) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref R14) (pin 1))
      (node (ref U1) (pin 1))
      (node (ref C28) (pin 2))
      (node (ref C26) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref C17) (pin 2))
      (node (ref C18) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref R15) (pin 1)))
    (net (code 7) (name "Net-(L3-Pad2)")
      (node (ref L3) (pin 2))
      (node (ref R19) (pin 1)))
    (net (code 8) (name "Net-(L5-Pad2)")
      (node (ref R21) (pin 1))
      (node (ref L5) (pin 2)))
    (net (code 9) (name "Net-(C24-Pad1)")
      (node (ref U3) (pin 5))
      (node (ref C24) (pin 1))
      (node (ref R22) (pin 2)))
    (net (code 10) (name "Net-(J2-Pad4)")
      (node (ref J2) (pin 4)))
    (net (code 11) (name "Net-(J2-Pad6)")
      (node (ref J2) (pin 6))
      (node (ref R16) (pin 1)))
    (net (code 12) (name +3V3)
      (node (ref C23) (pin 1))
      (node (ref U5) (pin 40))
      (node (ref R7) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref L2) (pin 2))
      (node (ref C25) (pin 1))
      (node (ref R10) (pin 1))
      (node (ref U5) (pin 28))
      (node (ref U5) (pin 29))
      (node (ref C27) (pin 1))
      (node (ref R54) (pin 2))
      (node (ref C29) (pin 1))
      (node (ref U4) (pin 22))
      (node (ref U4) (pin 4))
      (node (ref U4) (pin 41))
      (node (ref U4) (pin 43))
      (node (ref U4) (pin 31))
      (node (ref U4) (pin 9))
      (node (ref R23) (pin 1))
      (node (ref R24) (pin 1))
      (node (ref U5) (pin 11))
      (node (ref R9) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref R51) (pin 1)))
    (net (code 13) (name "Net-(R25-Pad1)")
      (node (ref R25) (pin 1))
      (node (ref U5) (pin 20)))
    (net (code 14) (name "Net-(R4-Pad1)")
      (node (ref R4) (pin 1))
      (node (ref U5) (pin 13)))
    (net (code 15) (name "Net-(R24-Pad2)")
      (node (ref U4) (pin 14))
      (node (ref U5) (pin 25))
      (node (ref R24) (pin 2)))
    (net (code 16) (name "Net-(U4-Pad18)")
      (node (ref U4) (pin 18))
      (node (ref U5) (pin 26)))
    (net (code 17) (name "Net-(U4-Pad16)")
      (node (ref U5) (pin 23))
      (node (ref U4) (pin 16)))
    (net (code 18) (name "Net-(R50-Pad1)")
      (node (ref U4) (pin 17))
      (node (ref U5) (pin 22))
      (node (ref R50) (pin 1)))
    (net (code 19) (name "Net-(U4-Pad28)")
      (node (ref U4) (pin 28))
      (node (ref U5) (pin 19)))
    (net (code 20) (name "Net-(U4-Pad35)")
      (node (ref U4) (pin 35))
      (node (ref U5) (pin 18)))
    (net (code 21) (name "Net-(U4-Pad34)")
      (node (ref U5) (pin 17))
      (node (ref U4) (pin 34)))
    (net (code 22) (name "Net-(U4-Pad33)")
      (node (ref U4) (pin 33))
      (node (ref U5) (pin 16)))
    (net (code 23) (name "Net-(U4-Pad32)")
      (node (ref U5) (pin 15))
      (node (ref U4) (pin 32)))
    (net (code 24) (name "Net-(R51-Pad2)")
      (node (ref U5) (pin 27))
      (node (ref R51) (pin 2))
      (node (ref R6) (pin 1)))
    (net (code 25) (name +5V)
      (node (ref L1) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref U12) (pin 5))
      (node (ref L3) (pin 1)))
    (net (code 26) (name "/Host Side/+")
      (node (ref J2) (pin 3))
      (node (ref U12) (pin 3)))
    (net (code 27) (name "/Host Side/-")
      (node (ref U12) (pin 1))
      (node (ref J2) (pin 2)))
    (net (code 28) (name "Net-(R54-Pad1)")
      (node (ref U4) (pin 38))
      (node (ref R54) (pin 1)))
    (net (code 29) (name "Net-(L1-Pad2)")
      (node (ref R17) (pin 1))
      (node (ref L1) (pin 2)))
    (net (code 30) (name "Net-(R6-Pad2)")
      (node (ref U4) (pin 21))
      (node (ref R6) (pin 2)))
    (net (code 31) (name "Net-(R23-Pad2)")
      (node (ref U4) (pin 15))
      (node (ref R23) (pin 2))
      (node (ref U5) (pin 24)))
    (net (code 32) (name "Net-(R4-Pad2)")
      (node (ref U4) (pin 36))
      (node (ref R4) (pin 2)))
    (net (code 33) (name "Net-(R5-Pad2)")
      (node (ref U4) (pin 37))
      (node (ref R5) (pin 2)))
    (net (code 34) (name +1.0V)
      (node (ref C15) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref C17) (pin 1))
      (node (ref U5) (pin 38))
      (node (ref U5) (pin 3))
      (node (ref U5) (pin 8))
      (node (ref C32) (pin 1))
      (node (ref U5) (pin 21))
      (node (ref L6) (pin 2)))
    (net (code 35) (name "/Host Side/MDI3+")
      (node (ref TR1) (pin 3))
      (node (ref U5) (pin 9)))
    (net (code 36) (name "/Host Side/MDI2-")
      (node (ref TR1) (pin 5))
      (node (ref U5) (pin 7)))
    (net (code 37) (name "/Host Side/MDI2+")
      (node (ref TR1) (pin 6))
      (node (ref U5) (pin 6)))
    (net (code 38) (name "/Host Side/MDI1-")
      (node (ref TR1) (pin 8))
      (node (ref U5) (pin 5)))
    (net (code 39) (name "/Host Side/MDI1+")
      (node (ref U5) (pin 4))
      (node (ref TR1) (pin 9)))
    (net (code 40) (name "/Host Side/MDI0-")
      (node (ref U5) (pin 2))
      (node (ref TR1) (pin 11)))
    (net (code 41) (name "Net-(R25-Pad2)")
      (node (ref R25) (pin 2))
      (node (ref U4) (pin 27)))
    (net (code 42) (name TD2+)
      (node (ref U7) (pin 4))
      (node (ref TR1) (pin 16)))
    (net (code 43) (name +3.3VI)
      (node (ref C50) (pin 1))
      (node (ref C53) (pin 1))
      (node (ref C55) (pin 1))
      (node (ref C58) (pin 1))
      (node (ref C46) (pin 1))
      (node (ref U9) (pin 5))
      (node (ref U9) (pin 15))
      (node (ref C48) (pin 1))
      (node (ref C64) (pin 1))
      (node (ref C62) (pin 2))
      (node (ref C63) (pin 2))
      (node (ref R35) (pin 1))
      (node (ref U7) (pin 28))
      (node (ref R37) (pin 1))
      (node (ref U7) (pin 11))
      (node (ref R30) (pin 1))
      (node (ref L8) (pin 2))
      (node (ref R48) (pin 1))
      (node (ref R39) (pin 1))
      (node (ref R41) (pin 1))
      (node (ref U10) (pin 22))
      (node (ref U10) (pin 31))
      (node (ref U10) (pin 9))
      (node (ref U10) (pin 43))
      (node (ref U10) (pin 41))
      (node (ref U10) (pin 4))
      (node (ref U7) (pin 29))
      (node (ref U7) (pin 40))
      (node (ref R56) (pin 1))
      (node (ref C40) (pin 1))
      (node (ref R52) (pin 1))
      (node (ref C38) (pin 1))
      (node (ref C43) (pin 1)))
    (net (code 44) (name TD4-)
      (node (ref U7) (pin 7))
      (node (ref TR1) (pin 23)))
    (net (code 45) (name TD4+)
      (node (ref U7) (pin 6))
      (node (ref TR1) (pin 22)))
    (net (code 46) (name TD3+)
      (node (ref TR1) (pin 19))
      (node (ref U7) (pin 9)))
    (net (code 47) (name TD3-)
      (node (ref TR1) (pin 20))
      (node (ref U7) (pin 10)))
    (net (code 48) (name "Net-(C64-Pad2)")
      (node (ref TR1) (pin 15))
      (node (ref C64) (pin 2))
      (node (ref TR1) (pin 21))
      (node (ref TR1) (pin 18))
      (node (ref TR1) (pin 24)))
    (net (code 49) (name TD2-)
      (node (ref TR1) (pin 17))
      (node (ref U7) (pin 5)))
    (net (code 50) (name TD1-)
      (node (ref U7) (pin 2))
      (node (ref TR1) (pin 14)))
    (net (code 51) (name TD1+)
      (node (ref U7) (pin 1))
      (node (ref TR1) (pin 13)))
    (net (code 52) (name D+)
      (node (ref U4) (pin 8))
      (node (ref U12) (pin 4)))
    (net (code 53) (name D-)
      (node (ref U12) (pin 6))
      (node (ref U4) (pin 7)))
    (net (code 54) (name "Net-(R18-Pad2)")
      (node (ref R18) (pin 2))
      (node (ref U1) (pin 2))
      (node (ref R3) (pin 1)))
    (net (code 55) (name "Net-(C9-Pad1)")
      (node (ref C9) (pin 1))
      (node (ref U1) (pin 3))
      (node (ref R17) (pin 2)))
    (net (code 56) (name "Net-(C12-Pad1)")
      (node (ref C12) (pin 1))
      (node (ref R3) (pin 2)))
    (net (code 57) (name "/Host Side/MDI3-")
      (node (ref U5) (pin 10))
      (node (ref TR1) (pin 2)))
    (net (code 58) (name "/Host Side/MDI0+")
      (node (ref U5) (pin 1))
      (node (ref TR1) (pin 12)))
    (net (code 59) (name "Net-(R10-Pad2)")
      (node (ref U5) (pin 32))
      (node (ref R10) (pin 2)))
    (net (code 60) (name "Net-(D2-Pad2)")
      (node (ref R12) (pin 2))
      (node (ref D2) (pin 2))
      (node (ref U5) (pin 34)))
    (net (code 61) (name "Net-(D2-Pad1)")
      (node (ref D2) (pin 1))
      (node (ref R14) (pin 2)))
    (net (code 62) (name "Net-(U5-Pad30)")
      (node (ref U5) (pin 30)))
    (net (code 63) (name "Net-(C23-Pad2)")
      (node (ref C23) (pin 2))
      (node (ref TR1) (pin 1))
      (node (ref TR1) (pin 7))
      (node (ref TR1) (pin 4))
      (node (ref TR1) (pin 10)))
    (net (code 64) (name "Net-(U5-Pad31)")
      (node (ref U5) (pin 31)))
    (net (code 65) (name "Net-(C19-Pad1)")
      (node (ref C19) (pin 1))
      (node (ref R9) (pin 2))
      (node (ref U5) (pin 12)))
    (net (code 66) (name "Net-(U5-Pad35)")
      (node (ref U5) (pin 35)))
    (net (code 67) (name "Net-(D1-Pad1)")
      (node (ref D1) (pin 1))
      (node (ref R13) (pin 2)))
    (net (code 68) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref R11) (pin 2))
      (node (ref U5) (pin 33)))
    (net (code 69) (name "Net-(R5-Pad1)")
      (node (ref R5) (pin 1))
      (node (ref R7) (pin 2))
      (node (ref U5) (pin 14)))
    (net (code 70) (name "Net-(R1-Pad1)")
      (node (ref R1) (pin 1))
      (node (ref U4) (pin 42)))
    (net (code 71) (name "Net-(R2-Pad1)")
      (node (ref R2) (pin 1))
      (node (ref U4) (pin 6)))
    (net (code 72) (name "Net-(C4-Pad1)")
      (node (ref Y1) (pin 1))
      (node (ref U4) (pin 3))
      (node (ref C4) (pin 1)))
    (net (code 73) (name "Net-(C3-Pad1)")
      (node (ref Y1) (pin 2))
      (node (ref U4) (pin 2))
      (node (ref C3) (pin 1)))
    (net (code 74) (name "Net-(C20-Pad1)")
      (node (ref C20) (pin 1))
      (node (ref Y2) (pin 2))
      (node (ref U5) (pin 36)))
    (net (code 75) (name "Net-(C21-Pad1)")
      (node (ref Y2) (pin 1))
      (node (ref U5) (pin 37))
      (node (ref C21) (pin 1)))
    (net (code 76) (name "Net-(C16-Pad1)")
      (node (ref R19) (pin 2))
      (node (ref C16) (pin 1))
      (node (ref U2) (pin 3)))
    (net (code 77) (name "Net-(R20-Pad2)")
      (node (ref U2) (pin 2))
      (node (ref R8) (pin 1))
      (node (ref R20) (pin 2)))
    (net (code 78) (name "Net-(C18-Pad1)")
      (node (ref R8) (pin 2))
      (node (ref C18) (pin 1)))
    (net (code 79) (name "Net-(R15-Pad2)")
      (node (ref R15) (pin 2))
      (node (ref U5) (pin 39)))
    (net (code 80) (name "Net-(C22-Pad1)")
      (node (ref U3) (pin 3))
      (node (ref U3) (pin 1))
      (node (ref R21) (pin 2))
      (node (ref C22) (pin 1)))
    (net (code 81) (name "Net-(U3-Pad4)")
      (node (ref U3) (pin 4)))
    (net (code 82) (name "Net-(R48-Pad2)")
      (node (ref R48) (pin 2))
      (node (ref U9) (pin 1)))
    (net (code 83) (name +1.0VI)
      (node (ref U7) (pin 21))
      (node (ref C44) (pin 1))
      (node (ref L12) (pin 2))
      (node (ref C41) (pin 1))
      (node (ref C39) (pin 1))
      (node (ref C37) (pin 1))
      (node (ref U7) (pin 8))
      (node (ref U7) (pin 38))
      (node (ref U7) (pin 3)))
    (net (code 84) (name "Net-(U10-Pad36)")
      (node (ref U9) (pin 3))
      (node (ref U10) (pin 36)))
    (net (code 85) (name "Net-(R42-Pad2)")
      (node (ref U10) (pin 21))
      (node (ref R42) (pin 2)))
    (net (code 86) (name "Net-(R43-Pad2)")
      (node (ref U10) (pin 27))
      (node (ref R43) (pin 2)))
    (net (code 87) (name "Net-(R41-Pad2)")
      (node (ref U10) (pin 15))
      (node (ref U7) (pin 24))
      (node (ref R41) (pin 2)))
    (net (code 88) (name "Net-(L12-Pad1)")
      (node (ref L12) (pin 1))
      (node (ref R45) (pin 1)))
    (net (code 89) (name "Net-(R38-Pad1)")
      (node (ref U8) (pin 2))
      (node (ref R38) (pin 1))
      (node (ref R40) (pin 2)))
    (net (code 90) (name "Net-(L10-Pad1)")
      (node (ref L10) (pin 1))
      (node (ref R40) (pin 1)))
    (net (code 91) (name "Net-(L8-Pad1)")
      (node (ref R34) (pin 1))
      (node (ref L8) (pin 1)))
    (net (code 92) (name "Net-(R33-Pad1)")
      (node (ref R33) (pin 1))
      (node (ref R34) (pin 2))
      (node (ref U6) (pin 2)))
    (net (code 93) (name +1.8VI)
      (node (ref C59) (pin 1))
      (node (ref L11) (pin 1))
      (node (ref L10) (pin 2))
      (node (ref C54) (pin 1))
      (node (ref C51) (pin 1))
      (node (ref C49) (pin 1))
      (node (ref U10) (pin 1))
      (node (ref U10) (pin 11))
      (node (ref U10) (pin 12))
      (node (ref C47) (pin 1))
      (node (ref U10) (pin 19))
      (node (ref U10) (pin 29))
      (node (ref U10) (pin 39))
      (node (ref C56) (pin 1)))
    (net (code 94) (name "Net-(C52-Pad1)")
      (node (ref R44) (pin 2))
      (node (ref C52) (pin 1))
      (node (ref U11) (pin 1))
      (node (ref U11) (pin 3)))
    (net (code 95) (name "Net-(C57-Pad1)")
      (node (ref U11) (pin 5))
      (node (ref C57) (pin 1))
      (node (ref R45) (pin 2)))
    (net (code 96) (name "Net-(C31-Pad1)")
      (node (ref U6) (pin 3))
      (node (ref R26) (pin 2))
      (node (ref C31) (pin 1)))
    (net (code 97) (name "Net-(J3-Pad5)")
      (node (ref R49) (pin 1))
      (node (ref J3) (pin 5)))
    (net (code 98) (name "Net-(C42-Pad1)")
      (node (ref U8) (pin 3))
      (node (ref R36) (pin 2))
      (node (ref C42) (pin 1)))
    (net (code 99) (name "Net-(C45-Pad1)")
      (node (ref C45) (pin 1))
      (node (ref R38) (pin 2)))
    (net (code 100) (name "Net-(C33-Pad1)")
      (node (ref R33) (pin 2))
      (node (ref C33) (pin 1)))
    (net (code 101) (name "Net-(U10-Pad33)")
      (node (ref U7) (pin 16))
      (node (ref U10) (pin 33)))
    (net (code 102) (name "Net-(U7-Pad13)")
      (node (ref U9) (pin 14))
      (node (ref U7) (pin 13)))
    (net (code 103) (name "Net-(U10-Pad18)")
      (node (ref U10) (pin 18))
      (node (ref U7) (pin 26)))
    (net (code 104) (name "Net-(U10-Pad16)")
      (node (ref U7) (pin 23))
      (node (ref U10) (pin 16)))
    (net (code 105) (name "Net-(R43-Pad1)")
      (node (ref U7) (pin 20))
      (node (ref R43) (pin 1)))
    (net (code 106) (name "Net-(U10-Pad28)")
      (node (ref U7) (pin 19))
      (node (ref U10) (pin 28)))
    (net (code 107) (name "Net-(U10-Pad35)")
      (node (ref U10) (pin 35))
      (node (ref U7) (pin 18)))
    (net (code 108) (name "Net-(U10-Pad34)")
      (node (ref U7) (pin 17))
      (node (ref U10) (pin 34)))
    (net (code 109) (name "Net-(U10-Pad32)")
      (node (ref U7) (pin 15))
      (node (ref U10) (pin 32)))
    (net (code 110) (name "Net-(R42-Pad1)")
      (node (ref R42) (pin 1))
      (node (ref U7) (pin 27))
      (node (ref R52) (pin 2)))
    (net (code 111) (name +5VI)
      (node (ref U13) (pin 5))
      (node (ref J4) (pin 1))
      (node (ref L9) (pin 1))
      (node (ref L7) (pin 1)))
    (net (code 112) (name "Net-(J3-Pad1)")
      (node (ref J3) (pin 1)))
    (net (code 113) (name "Net-(L7-Pad2)")
      (node (ref R26) (pin 1))
      (node (ref L7) (pin 2)))
    (net (code 114) (name "Net-(R55-Pad1)")
      (node (ref U10) (pin 38))
      (node (ref R55) (pin 1)))
    (net (code 115) (name "Net-(R56-Pad2)")
      (node (ref R56) (pin 2))
      (node (ref U10) (pin 37))
      (node (ref U9) (pin 4)))
    (net (code 116) (name "Net-(R53-Pad1)")
      (node (ref U10) (pin 17))
      (node (ref U7) (pin 22))
      (node (ref R53) (pin 1)))
    (net (code 117) (name "/Device Side/D-")
      (node (ref J3) (pin 2))
      (node (ref U13) (pin 1)))
    (net (code 118) (name "/Device Side/D+")
      (node (ref J3) (pin 3))
      (node (ref U13) (pin 3)))
    (net (code 119) (name D2+)
      (node (ref U13) (pin 4))
      (node (ref U9) (pin 11))
      (node (ref U10) (pin 8)))
    (net (code 120) (name D2-)
      (node (ref U9) (pin 16))
      (node (ref U13) (pin 6))
      (node (ref U10) (pin 7)))
    (net (code 121) (name "Net-(TP1-Pad1)")
      (node (ref TP1) (pin 1))
      (node (ref U9) (pin 2)))
    (net (code 122) (name "Net-(L11-Pad2)")
      (node (ref R44) (pin 1))
      (node (ref L11) (pin 2)))
    (net (code 123) (name "Net-(L9-Pad2)")
      (node (ref R36) (pin 1))
      (node (ref L9) (pin 2)))
    (net (code 124) (name "Net-(C61-Pad1)")
      (node (ref C61) (pin 1))
      (node (ref U10) (pin 3))
      (node (ref Y4) (pin 1)))
    (net (code 125) (name "Net-(C60-Pad1)")
      (node (ref U10) (pin 2))
      (node (ref Y4) (pin 2))
      (node (ref C60) (pin 1)))
    (net (code 126) (name "Net-(R46-Pad1)")
      (node (ref R46) (pin 1))
      (node (ref U10) (pin 42)))
    (net (code 127) (name "Net-(R47-Pad1)")
      (node (ref U10) (pin 6))
      (node (ref R47) (pin 1)))
    (net (code 128) (name "Net-(U11-Pad4)")
      (node (ref U11) (pin 4)))
    (net (code 129) (name "Net-(D3-Pad1)")
      (node (ref R28) (pin 2))
      (node (ref D3) (pin 1)))
    (net (code 130) (name "Net-(U7-Pad30)")
      (node (ref U7) (pin 30)))
    (net (code 131) (name "Net-(C36-Pad1)")
      (node (ref R35) (pin 2))
      (node (ref U7) (pin 12))
      (node (ref C36) (pin 1)))
    (net (code 132) (name "Net-(R37-Pad2)")
      (node (ref R37) (pin 2))
      (node (ref U7) (pin 14))
      (node (ref U9) (pin 13)))
    (net (code 133) (name "Net-(C34-Pad1)")
      (node (ref Y3) (pin 2))
      (node (ref U7) (pin 36))
      (node (ref C34) (pin 1)))
    (net (code 134) (name "Net-(C35-Pad1)")
      (node (ref U7) (pin 37))
      (node (ref C35) (pin 1))
      (node (ref Y3) (pin 1)))
    (net (code 135) (name "Net-(U7-Pad31)")
      (node (ref U7) (pin 31)))
    (net (code 136) (name "Net-(U7-Pad35)")
      (node (ref U7) (pin 35)))
    (net (code 137) (name "Net-(D4-Pad1)")
      (node (ref D4) (pin 1))
      (node (ref R29) (pin 2)))
    (net (code 138) (name "Net-(D3-Pad2)")
      (node (ref U7) (pin 34))
      (node (ref D3) (pin 2))
      (node (ref R32) (pin 2)))
    (net (code 139) (name GND2)
      (node (ref C50) (pin 2))
      (node (ref C54) (pin 2))
      (node (ref C33) (pin 2))
      (node (ref C52) (pin 2))
      (node (ref C43) (pin 2))
      (node (ref C31) (pin 2))
      (node (ref C38) (pin 2))
      (node (ref C40) (pin 2))
      (node (ref C48) (pin 2))
      (node (ref C47) (pin 2))
      (node (ref C55) (pin 2))
      (node (ref C58) (pin 2))
      (node (ref C53) (pin 2))
      (node (ref C59) (pin 2))
      (node (ref C56) (pin 2))
      (node (ref R49) (pin 2))
      (node (ref C39) (pin 2))
      (node (ref U9) (pin 8))
      (node (ref C49) (pin 2))
      (node (ref U6) (pin 1))
      (node (ref C46) (pin 2))
      (node (ref C51) (pin 2))
      (node (ref C44) (pin 2))
      (node (ref C41) (pin 2))
      (node (ref C37) (pin 2))
      (node (ref R55) (pin 2))
      (node (ref J3) (pin 4))
      (node (ref U10) (pin 25))
      (node (ref U11) (pin 2))
      (node (ref U8) (pin 1))
      (node (ref C42) (pin 2))
      (node (ref C45) (pin 2))
      (node (ref U10) (pin 13))
      (node (ref U10) (pin 10))
      (node (ref U10) (pin 20))
      (node (ref R27) (pin 1))
      (node (ref R31) (pin 1))
      (node (ref R32) (pin 1))
      (node (ref R29) (pin 1))
      (node (ref C36) (pin 2))
      (node (ref C35) (pin 2))
      (node (ref C34) (pin 2))
      (node (ref R28) (pin 1))
      (node (ref R47) (pin 2))
      (node (ref J4) (pin 2))
      (node (ref U13) (pin 2))
      (node (ref R53) (pin 2))
      (node (ref R46) (pin 2))
      (node (ref C61) (pin 2))
      (node (ref U10) (pin 30))
      (node (ref C60) (pin 2))
      (node (ref U10) (pin 5))
      (node (ref U10) (pin 44))
      (node (ref U10) (pin 40))
      (node (ref C63) (pin 1))
      (node (ref C62) (pin 1))
      (node (ref U7) (pin 41))
      (node (ref C57) (pin 2)))
    (net (code 140) (name "Net-(D4-Pad2)")
      (node (ref D4) (pin 2))
      (node (ref R31) (pin 2))
      (node (ref U7) (pin 33)))
    (net (code 141) (name "Net-(R39-Pad2)")
      (node (ref U10) (pin 14))
      (node (ref U7) (pin 25))
      (node (ref R39) (pin 2)))
    (net (code 142) (name "Net-(R30-Pad2)")
      (node (ref U7) (pin 32))
      (node (ref R30) (pin 2)))
    (net (code 143) (name "Net-(R27-Pad2)")
      (node (ref U7) (pin 39))
      (node (ref R27) (pin 2)))
    (net (code 144) (name "Net-(U9-Pad10)")
      (node (ref U9) (pin 10)))
    (net (code 145) (name "Net-(U9-Pad9)")
      (node (ref U9) (pin 9)))
    (net (code 146) (name "Net-(U9-Pad7)")
      (node (ref U9) (pin 7)))
    (net (code 147) (name "Net-(U9-Pad6)")
      (node (ref U9) (pin 6)))
    (net (code 148) (name "Net-(U9-Pad12)")
      (node (ref U9) (pin 12)))))