EESchema-DOCLIB  Version 2.0
#
$CMP +5V_SW
D Power symbol creates a global label with name "+5V_SW"
K power-flag
$ENDCMP
#
$CMP 25LCxxx
D SPI Serial EEPROM, DIP-8/SOIC-8/TSSOP-8
K EEPROM memory SPI serial
F http://ww1.microchip.com/downloads/en/DeviceDoc/21832H.pdf
$ENDCMP
#
$CMP 74LVC2G66
D Dual Analog Switches
K CMOS SWITCH
F https://assets.nexperia.com/documents/data-sheet/74LVC2G66.pdf
$ENDCMP
#
$CMP AT25xxx
D Microchip SPI Serial EEPROM, DIP-8/SOIC-8/TSSOP-8
K EEPROM memory SPI serial
F http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8707-SEEPROM-AT25010B-020B-040B-Datasheet.pdf
$ENDCMP
#
$CMP BR25Sxxx
D ROHM Semiconductor SPI Serial EEPROM, DIP-8/SOIC-8/TSSOP-8
K EEPROM memory SPI serial
F http://www.rohm.com/web/global/products/-/product/BR25G128F-3
$ENDCMP
#
$CMP CAT250xxx
D ON Semiconductor SPI Serial EEPROM, DIP-8/SOIC-8/TSSOP-8
K EEPROM memory SPI serial
F http://www.onsemi.com/PowerSolutions/product.do?id=CAT25040
$ENDCMP
#
$CMP ESD7104
D Low Capacitance ESD Protection Diodefor High Speed Data Line, 2 Channels, UDFN-10/WDFNW-10
K ESD protection suppression transient USB HDMI eSATA DisplayPort Thunderbolt
F https://www.onsemi.com/pub/Collateral/ESD7104-D.PDF
$ENDCMP
#
$CMP HD3SS3220
D USB Type-C DRP Port Controller with SuperSpeed 2:1 MUX, Texas Instruments, VQFN-30
K usb usb-c type-c mux
$ENDCMP
#
$CMP TPS2061C
D 1.0A, 4.5-5.5V USB power switch, active-low enable, output discharge
K 1-chanel power-distribution USB
F https://www.ti.com/lit/gpn/tps2061c
$ENDCMP
#
$CMP TS3A24157
D Dual SPDT 0.65Ω Bidirectional Analog Switch, VSSOP-10
K switch analog SPDT
F http://www.ti.com/lit/ds/symlink/ts3a24159.pdf
$ENDCMP
#
$CMP USB3_B
D USB 3.0 B connector
K usb universal serial bus
F ~
$ENDCMP
#
$CMP USB_C_Receptacle
D USB Full-Featured Type-C Receptacle connector
K usb universal serial bus type-C full-featured
F https://www.usb.org/sites/default/files/documents/usb_type-c.zip
$ENDCMP
#
$CMP VL670
D USB 3 Super Speed to USB 2 High Speed Transaction Translator, VIA Labs, QFN-48
K usb
$ENDCMP
#
#End Doc Library
