# config.links - helper for ../configure             -*- mode: sh -*-
# Copyright (C) 1998, 1999, 2000, 2001, 2002 Free Software Foundation, Inc.
#
# This file is part of Libgcrypt.
#
# Libgcrypt is free software; you can redistribute it and/or modify
# it under the terms of the GNU Lesser General Public License as
# published by the Free Software Foundation; either version 2.1 of
# the License, or (at your option) any later version.
#
# Libgcrypt is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU Lesser General Public License for more details.
#
# You should have received a copy of the GNU Lesser General Public
# License along with this program; if not, write to the Free Software
# Foundation, Inc., 59 Temple Place - Suite 330, Boston, MA 02111-1307, USA
#
# sourced by ../configure to get the list of files to link
# this should set $mpi_ln_list.
# Note: this is called from the above directory.

mpi_sflags=
mpi_extra_modules=

test -d ./mpi || mkdir ./mpi

# We grep the list of modules from the Makefile so that
# we don't need to maintain them here.
mpi_standard_modules=`$AWK '/^#BEGIN_ASM_LIST/,/^#END_ASM_LIST/ {
                 if( $3 != "O" ) print $2 }'  $srcdir/mpi/Makefile.am`
mpi_optional_modules=`$AWK '/^#BEGIN_ASM_LIST/,/^#END_ASM_LIST/ {
                 if( $3 == "O" ) print $2 }' $srcdir/mpi/Makefile.am`


echo '/* created by config.links - do not edit */' >./mpi/asm-syntax.h
echo "/* Host: ${host} */" >>./mpi/asm-syntax.h

if test "$try_asm_modules" = "yes" ; then
case "${host}" in
    powerpc-apple-darwin*          | \
    i[34567]86*-*-openbsd[12]*     | \
    i[34567]86*-*-openbsd3.[0123]*)
       echo '/* No working assembler modules available */' >>./mpi/asm-syntax.h
       path=""
       ;;
    i[3467]86*-*-openbsd*      | \
    i[3467]86*-*-freebsd*-elf  | \
    i[3467]86*-*-freebsd[3-9]* | \
    i[3467]86*-*-freebsdelf*   | \
    i[3467]86*-*-netbsd*       | \
    i[3467]86*-*-k*bsd*)
       echo '#define ELF_SYNTAX' >>./mpi/asm-syntax.h
       cat  $srcdir/mpi/i386/syntax.h	   >>./mpi/asm-syntax.h
       path="i386"
       ;;
    i586*-*-openbsd*         | \
    i586*-*-freebsd*-elf     | \
    i586*-*-freebsd[3-9]*    | \
    i586*-*-freebsdelf*      | \
    i586*-*-netbsd*	     | \
    i586*-*-k*bsd*	     | \
    pentium-*-netbsd*	     | \
    pentiumpro-*-netbsd*)
       echo '#define ELF_SYNTAX' >>./mpi/asm-syntax.h
       cat  $srcdir/mpi/i386/syntax.h	   >>./mpi/asm-syntax.h
       path="i586 i386"
       ;;
    i[34]86*-*-bsdi4*)
       echo '#define ELF_SYNTAX' >>./mpi/asm-syntax.h
       cat  $srcdir/mpi/i386/syntax.h	 >>./mpi/asm-syntax.h
       path="i386"
       ;;
    i[3467]86*-*-linuxaout*  | \
    i[3467]86*-*-linuxoldld* | \
    i[3467]86*-*-*bsd*)
	echo '#define BSD_SYNTAX' >>./mpi/asm-syntax.h
	echo '#define X86_BROKEN_ALIGN' >>./mpi/asm-syntax.h
	cat  $srcdir/mpi/i386/syntax.h	    >>./mpi/asm-syntax.h
	path="i386"
	;;
    i586*-*-linuxaout*  | \
    i586*-*-linuxoldld* | \
    i586*-*-*bsd*)
	echo '#define BSD_SYNTAX' >>./mpi/asm-syntax.h
	echo '#define X86_BROKEN_ALIGN' >>./mpi/asm-syntax.h
	cat  $srcdir/mpi/i386/syntax.h	    >>./mpi/asm-syntax.h
	path="i586 i386"
	;;
    i[3467]86*-msdosdjgpp* | \
    i[34]86*-apple-darwin*)
	echo '#define BSD_SYNTAX'        >>./mpi/asm-syntax.h
	cat  $srcdir/mpi/i386/syntax.h	 >>./mpi/asm-syntax.h
	path="i386"
	;;
    i586*-msdosdjgpp* | \
    i[567]86*-apple-darwin*)
	echo '#define BSD_SYNTAX'        >>./mpi/asm-syntax.h
	cat  $srcdir/mpi/i386/syntax.h	 >>./mpi/asm-syntax.h
	path="i586 i386"
	;;
    i[3467]86*-*-*)
	echo '#define ELF_SYNTAX' >>./mpi/asm-syntax.h
	cat  $srcdir/mpi/i386/syntax.h	    >>./mpi/asm-syntax.h
	path="i386"
	;;
    i586*-*-*  | \
    pentium-*-*   | \
    pentiumpro-*-*)
	echo '#define ELF_SYNTAX' >>./mpi/asm-syntax.h
	cat  $srcdir/mpi/i386/syntax.h	    >>./mpi/asm-syntax.h
	path="i586 i386"
	;;
    x86_64-*-*)
	echo '#define ELF_SYNTAX' >>./mpi/asm-syntax.h
	cat  $srcdir/mpi/i386/syntax.h	    >>./mpi/asm-syntax.h
	path="amd64"
	;;
    alpha*-*-*)
	echo '/* configured for alpha */' >>./mpi/asm-syntax.h
	path="alpha"
	mpi_extra_modules="udiv-qrnnd"
	;;
    hppa7000*-*-*)
	echo '/* configured for HPPA (pa7000) */' >>./mpi/asm-syntax.h
	path="hppa1.1 hppa"
	mpi_extra_modules="udiv-qrnnd"
	;;
    hppa1.0*-*-*)
	echo '/* configured for HPPA 1.0 */' >>./mpi/asm-syntax.h
	path="hppa"
	mpi_extra_modules="udiv-qrnnd"
	;;
    hppa*-*-*)	# assume pa7100
	echo '/* configured for HPPA (pa7100) */' >>./mpi/asm-syntax.h
	path="pa7100 hppa1.1 hppa"
	mpi_extra_modules="udiv-qrnnd"
	;;
    sparc64-*-linux-gnu)
        echo '/* No working assembler modules available */' >>./mpi/asm-syntax.h
	path=""
	;;
    sparc64-sun-solaris2*)
        echo '/* No working assembler modules available */' >>./mpi/asm-syntax.h
	path=""
        ;;
    sparc64-*-netbsd* | sparc64-*-freebsd* | sparc64-*-openbsd*)
       # There are no sparc64 assembler modules that work on the
       # *BSDs, so use the generic C functions.
       echo '/* No working assembler modules available */' >>./mpi/asm-syntax.h
       path=""
       ;;
    sparc64*-*-*)
       echo '/* No working assembler modules available */' >>./mpi/asm-syntax.h
       path=""
       ;;
    sparc9*-*-*     | \
    ultrasparc*-*-* )
	echo '/* configured for sparc9 or higher */' >>./mpi/asm-syntax.h
	path="sparc32v8 sparc32"
	;;
    sparc8*-*-*     | \
    microsparc*-*-*)
	echo '/* configured for sparc8 */' >>./mpi/asm-syntax.h
	path="sparc32v8 sparc32"
	;;
    supersparc*-*-*)
	echo '/* configured for supersparc */' >>./mpi/asm-syntax.h
	path="supersparc sparc32v8 sparc32"
	mpi_extra_modules="udiv"
	;;
    sparc*-*-*)
	echo '/* configured for sparc */' >>./mpi/asm-syntax.h
	path="sparc32"
	mpi_extra_modules="udiv"
	;;
    mips[34]*-*-* | \
    mips*-*-irix6*)
       echo '/* configured for MIPS3 */' >>./mpi/asm-syntax.h
       path="mips3"
       ;;
    mips*-*-*)
       echo '/* configured for MIPS2 */' >>./mpi/asm-syntax.h
       path="mips2"
       ;;

    # Motorola 68k configurations.  Let m68k mean 68020-68040.
    # mc68000 or mc68060 configurations need to be specified explicitly
    m680[234]0*-*-linuxaout* | \
    m68k*-*-linuxaout*)
	echo '#define MIT_SYNTAX'           >>./mpi/asm-syntax.h
	cat  $srcdir/mpi/m68k/syntax.h	    >>./mpi/asm-syntax.h
	path="m68k/mc68020 m68k"
	;;
    m68060*-*-linuxaout*)
	echo '#define MIT_SYNTAX'           >>./mpi/asm-syntax.h
	cat  $srcdir/mpi/m68k/syntax.h	    >>./mpi/asm-syntax.h
	path="m68k"
	;;
    m680[234]0*-*-linux* | \
    m68k*-*-linux*)
	echo '#define ELF_SYNTAX'           >>./mpi/asm-syntax.h
	cat  $srcdir/mpi/m68k/syntax.h	    >>./mpi/asm-syntax.h
	;;
    m68060*-*-linux*)
	echo '#define ELF_SYNTAX'           >>./mpi/asm-syntax.h
	cat  $srcdir/mpi/m68k/syntax.h	    >>./mpi/asm-syntax.h
	path="m68k"
	;;
    m68k-atari-mint)
	echo '#define MIT_SYNTAX'           >>./mpi/asm-syntax.h
	cat  $srcdir/mpi/m68k/syntax.h	    >>./mpi/asm-syntax.h
	path="m68k/mc68020 m68k"
	;;
    m68000*-*-* | \
    m68060*-*-*)
	echo '#define MIT_SYNTAX'           >>./mpi/asm-syntax.h
	cat  $srcdir/mpi/m68k/syntax.h	    >>./mpi/asm-syntax.h
	path="m68k/mc68000"
	;;
    m680[234]0*-*-* | \
    m68k*-*-*)
	echo '#define MIT_SYNTAX'           >>./mpi/asm-syntax.h
	cat  $srcdir/mpi/m68k/syntax.h	    >>./mpi/asm-syntax.h
	path="m68k/mc68020 m68k"
	;;

    powerpc*-*-netbsd* | powerpc*-*-openbsd*)
       echo '/* configured {Open,Net}BSD on powerpc */' >>./mpi/asm-syntax.h
       echo '#define ELF_SYNTAX'                 >>./mpi/asm-syntax.h
       cat   $srcdir/mpi/powerpc32/syntax.h	 >>./mpi/asm-syntax.h
       mpi_sflags="-Wa,-mppc"
       path="powerpc32"
       ;;

    ppc620-*-*	    | \
    powerpc64*-*-*)
	mpi_sflags="-Wa,-mppc"
	path="powerpc64"
	;;
    powerpc*-*-linux*)
	echo '/* configured for powerpc/ELF */' >>./mpi/asm-syntax.h
	echo '#define ELF_SYNTAX'               >>./mpi/asm-syntax.h
	cat   $srcdir/mpi/powerpc32/syntax.h	>>./mpi/asm-syntax.h
	path="powerpc32"
	;;

    rs6000-*-aix[456789]*    | \
    rs6000-*-aix3.2.[456789])
	mpi_sflags="-Wa,-mpwr"
	path="power"
	mpi_extra_modules="udiv-w-sdiv"
	;;
    rs6000-*-* | \
    power-*-*  | \
    power2-*-*)
	mpi_sflags="-Wa,-mppc"
	path="power"
	mpi_extra_modules="udiv-w-sdiv"
	;;
    powerpc-ibm-aix4.2.* )
	# I am not sure about this one but a machine identified by
	# powerpc-ibm-aix4.2.1.0 cannot use the powerpc32 code.
	mpi_sflags="-Wa,-mpwr"
	path="power"
	mpi_extra_modules="udiv-w-sdiv"
	;;
    ppc601-*-*)
	mpi_sflags="-Wa,-mppc"
	path="power powerpc32"
	;;
    ppc60[234]*-*-*)
	mpi_sflags="-Wa,-mppc"
	path="powerpc32"
	;;
    powerpc*-*-*)
	mpi_sflags="-Wa,-mppc"
	path="powerpc32"
	;;
    *)
	echo '/* No assembler modules configured */' >>./mpi/asm-syntax.h
	path=""
	;;
esac
else
    echo '/* Assembler modules disabled on request */' >>./mpi/asm-syntax.h
    path=""
fi


# Make sysdep.h
echo '/* created by config.links - do not edit */' >./mpi/sysdep.h
if test x$ac_cv_sys_symbol_underscore = xyes; then
    cat <<EOF >>./mpi/sysdep.h
#if __STDC__
#define C_SYMBOL_NAME(name) _##name
#else
#define C_SYMBOL_NAME(name) _/**/name
#endif
EOF
else
    cat <<EOF >>./mpi/sysdep.h
#define C_SYMBOL_NAME(name) name
EOF
fi


# Figure the required modules out
mpi_required_modules=$mpi_standard_modules
if test "$mpi_extra_modules" != ""; then
  for fn in $mpi_extra_modules; do
      for i in $mpi_optional_modules; do
          if test "$fn" = "$i" ; then
             mpi_required_modules="$mpi_required_modules $fn"
          fi
      done
  done
fi

# Try to get file to link from the assembler subdirectory and
# if this fails get it from the generic subdirectory.
mpi_ln_list=
mpi_mod_list=
path=`echo "$mpi_extra_path $path generic" | tr ':' ' '`
echo '/* Created by config.links - do not edit */' >./mpi/mod-source-info.h
echo "/* Host: ${host} */" >>./mpi/mod-source-info.h
echo "static char mod_source_info[] =" >>./mpi/mod-source-info.h
for fn in $mpi_required_modules ; do
    fnu=`echo $fn | sed 's/-/_/g'`
    eval mpi_mod_c_${fnu}=no
    eval mpi_mod_asm_${fnu}=no
    for dir in $path ; do
	rm -f $srcdir/mpi/$fn.[Sc]
	if test -f $srcdir/mpi/$dir/$fn.S ; then
            echo "  \":$dir/$fn.S\"" >>./mpi/mod-source-info.h
            mpi_ln_list="$mpi_ln_list mpi/$fn-asm.S:mpi/$dir/$fn.S"
            eval mpi_mod_asm_${fnu}=yes
            mpi_mod_list="$mpi_mod_list $fn"
	    break;
	elif test -f $srcdir/mpi/$dir/$fn.c ; then
            echo "  \":$dir/$fn.c\"" >>./mpi/mod-source-info.h
            mpi_ln_list="$mpi_ln_list mpi/$fn.c:mpi/$dir/$fn.c"
            eval mpi_mod_c_${fnu}=yes
            mpi_mod_list="$mpi_mod_list $fn"
	    break;
	fi
    done
done
echo "  ;" >>./mpi/mod-source-info.h

# Same thing for the file which defines the limb size
path=`echo "$path generic" | tr ':' ' '`
for dir in $path ; do
    rm -f $srcdir/mpi/mpi-asm-defs.h
    if test -f $srcdir/mpi/$dir/mpi-asm-defs.h ; then
        mpi_ln_list="$mpi_ln_list mpi/mpi-asm-defs.h:mpi/$dir/mpi-asm-defs.h"
        break;
    fi
done
