From f536a600e0e20fd57475415ce5b3d909441d53b6 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Sun, 10 Jan 2016 17:31:46 +0100
Subject: [PATCH 046/102] regulator: Add document for MT6323 regulator

Signed-off-by: John Crispin <blogic@openwrt.org>
Cc: devicetree@vger.kernel.org
---
 .../bindings/regulator/mt6323-regulator.txt        |  239 ++++++++++++++++++++
 1 file changed, 239 insertions(+)
 create mode 100644 Documentation/devicetree/bindings/regulator/mt6323-regulator.txt

--- /dev/null
+++ b/Documentation/devicetree/bindings/regulator/mt6323-regulator.txt
@@ -0,0 +1,239 @@
+Mediatek MT6323 Regulator Driver
+
+All voltage regulators are defined as subnodes of the regulators node. A list
+of regulators provided by this controller are defined as subnodes of the
+PMIC's node. Each regulator is named according to its regulator type,
+buck_<name> and ldo_<name>. The definition for each of these nodes is defined
+using the standard binding for regulators at
+Documentation/devicetree/bindings/regulator/regulator.txt.
+
+The valid names for regulators are::
+BUCK:
+  buck_vproc, buck_vsys, buck_vpa
+LDO:
+  ldo_vtcxo, ldo_vcn28, ldo_vcn33_bt, ldo_vcn33_wifi, ldo_va, ldo_vcama,
+  ldo_vio28, ldo_vusb, ldo_vmc, ldo_vmch, ldo_vemc3v3, ldo_vgp1, ldo_vgp2,
+  ldo_vgp3, ldo_vcn18, ldo_vsim1, ldo_vsim2, ldo_vrtc, ldo_vcamaf, ldo_vibr,
+  ldo_vrf18, ldo_vm, ldo_vio18, ldo_vcamd, ldo_vcamio
+
+Example:
+
+	pmic: mt6323 {
+		compatible = "mediatek,mt6323";
+
+		mt6323regulator: regulators {
+			mt6323_vproc_reg: buck_vproc{
+				regulator-name = "vproc";
+				regulator-min-microvolt = < 700000>;
+				regulator-max-microvolt = <1350000>;
+				regulator-ramp-delay = <12500>;
+				regulator-always-on;
+				regulator-boot-on;
+			};
+
+			mt6323_vsys_reg: buck_vsys{
+				regulator-name = "vsys";
+				regulator-min-microvolt = <1400000>;
+				regulator-max-microvolt = <2987500>;
+				regulator-ramp-delay = <25000>;
+				regulator-always-on;
+				regulator-boot-on;
+			};
+
+			mt6323_vpa_reg: buck_vpa{
+				regulator-name = "vpa";
+				regulator-min-microvolt = < 500000>;
+				regulator-max-microvolt = <3650000>;
+			};
+
+			mt6323_vtcxo_reg: ldo_vtcxo{
+				regulator-name = "vtcxo";
+				regulator-min-microvolt = <2800000>;
+				regulator-max-microvolt = <2800000>;
+				regulator-enable-ramp-delay = <90>;
+				regulator-always-on;
+				regulator-boot-on;
+			};
+
+			mt6323_vcn28_reg: ldo_vcn28{
+				regulator-name = "vcn28";
+				regulator-min-microvolt = <2800000>;
+				regulator-max-microvolt = <2800000>;
+				regulator-enable-ramp-delay = <185>;
+			};
+
+			mt6323_vcn33_bt_reg: ldo_vcn33_bt{
+				regulator-name = "vcn33_bt";
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3600000>;
+				regulator-enable-ramp-delay = <185>;
+			};
+
+			mt6323_vcn33_wifi_reg: ldo_vcn33_wifi{
+				regulator-name = "vcn33_wifi";
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3600000>;
+				regulator-enable-ramp-delay = <185>;
+			};
+
+			mt6323_va_reg: ldo_va{
+				regulator-name = "va";
+				regulator-min-microvolt = <2800000>;
+				regulator-max-microvolt = <2800000>;
+				regulator-enable-ramp-delay = <216>;
+				regulator-always-on;
+				regulator-boot-on;
+			};
+
+			mt6323_vcama_reg: ldo_vcama{
+				regulator-name = "vcama";
+				regulator-min-microvolt = <1500000>;
+				regulator-max-microvolt = <2800000>;
+				regulator-enable-ramp-delay = <216>;
+			};
+
+			mt6323_vio28_reg: ldo_vio28{
+				regulator-name = "vio28";
+				regulator-min-microvolt = <2800000>;
+				regulator-max-microvolt = <2800000>;
+				regulator-enable-ramp-delay = <216>;
+				regulator-always-on;
+				regulator-boot-on;
+			};
+
+			mt6323_vusb_reg: ldo_vusb{
+				regulator-name = "vusb";
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-enable-ramp-delay = <216>;
+				regulator-boot-on;
+			};
+
+			mt6323_vmc_reg: ldo_vmc{
+				regulator-name = "vmc";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-enable-ramp-delay = <36>;
+				regulator-boot-on;
+			};
+
+			mt6323_vmch_reg: ldo_vmch{
+				regulator-name = "vmch";
+				regulator-min-microvolt = <3000000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-enable-ramp-delay = <36>;
+				regulator-boot-on;
+			};
+
+			mt6323_vemc3v3_reg: ldo_vemc3v3{
+				regulator-name = "vemc3v3";
+				regulator-min-microvolt = <3000000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-enable-ramp-delay = <36>;
+				regulator-boot-on;
+			};
+
+			mt6323_vgp1_reg: ldo_vgp1{
+				regulator-name = "vgp1";
+				regulator-min-microvolt = <1200000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-enable-ramp-delay = <216>;
+			};
+
+			mt6323_vgp2_reg: ldo_vgp2{
+				regulator-name = "vgp2";
+				regulator-min-microvolt = <1200000>;
+				regulator-max-microvolt = <3000000>;
+				regulator-enable-ramp-delay = <216>;
+			};
+
+			mt6323_vgp3_reg: ldo_vgp3{
+				regulator-name = "vgp3";
+				regulator-min-microvolt = <1200000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-enable-ramp-delay = <216>;
+			};
+
+			mt6323_vcn18_reg: ldo_vcn18{
+				regulator-name = "vcn18";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-enable-ramp-delay = <216>;
+			};
+
+			mt6323_vsim1_reg: ldo_vsim1{
+				regulator-name = "vsim1";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <3000000>;
+				regulator-enable-ramp-delay = <216>;
+			};
+
+			mt6323_vsim2_reg: ldo_vsim2{
+				regulator-name = "vsim2";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <3000000>;
+				regulator-enable-ramp-delay = <216>;
+			};
+
+			mt6323_vrtc_reg: ldo_vrtc{
+				regulator-name = "vrtc";
+				regulator-min-microvolt = <2800000>;
+				regulator-max-microvolt = <2800000>;
+				regulator-always-on;
+				regulator-boot-on;
+			};
+
+			mt6323_vcamaf_reg: ldo_vcamaf{
+				regulator-name = "vcamaf";
+				regulator-min-microvolt = <1200000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-enable-ramp-delay = <216>;
+			};
+
+			mt6323_vibr_reg: ldo_vibr{
+				regulator-name = "vibr";
+				regulator-min-microvolt = <1200000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-enable-ramp-delay = <36>;
+			};
+
+			mt6323_vrf18_reg: ldo_vrf18{
+				regulator-name = "vrf18";
+				regulator-min-microvolt = <1825000>;
+				regulator-max-microvolt = <1825000>;
+				regulator-enable-ramp-delay = <187>;
+			};
+
+			mt6323_vm_reg: ldo_vm{
+				regulator-name = "vm";
+				regulator-min-microvolt = <1200000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-enable-ramp-delay = <216>;
+				regulator-always-on;
+				regulator-boot-on;
+			};
+
+			mt6323_vio18_reg: ldo_vio18{
+				regulator-name = "vio18";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-enable-ramp-delay = <216>;
+				regulator-always-on;
+				regulator-boot-on;
+			};
+
+			mt6323_vcamd_reg: ldo_vcamd{
+				regulator-name = "vcamd";
+				regulator-min-microvolt = <1200000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-enable-ramp-delay = <216>;
+			};
+
+			mt6323_vcamio_reg: ldo_vcamio{
+				regulator-name = "vcamio";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-enable-ramp-delay = <216>;
+			};
+		};
+	};
