From 57c00f2fac512837f8de73474ec1f54020015bae Mon Sep 17 00:00:00 2001
From: Christophe Jaillet <christophe.jaillet@wanadoo.fr>
Date: Wed, 21 Jun 2017 07:45:53 +0200
Subject: [PATCH] brcmfmac: Fix a memory leak in error handling path in
 'brcmf_cfg80211_attach'

If 'wiphy_new()' fails, we leak 'ops'. Add a new label in the error
handling path to free it in such a case.

Cc: stable@vger.kernel.org
Fixes: 5c22fb85102a7 ("brcmfmac: add wowl gtk rekeying offload support")
Signed-off-by: Christophe JAILLET <christophe.jaillet@wanadoo.fr>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c
@@ -6842,7 +6842,7 @@ struct brcmf_cfg80211_info *brcmf_cfg802
 	wiphy = wiphy_new(ops, sizeof(struct brcmf_cfg80211_info));
 	if (!wiphy) {
 		brcmf_err("Could not allocate wiphy device\n");
-		return NULL;
+		goto ops_out;
 	}
 	memcpy(wiphy->perm_addr, drvr->mac, ETH_ALEN);
 	set_wiphy_dev(wiphy, busdev);
@@ -6985,6 +6985,7 @@ priv_out:
 	ifp->vif = NULL;
 wiphy_out:
 	brcmf_free_wiphy(wiphy);
+ops_out:
 	kfree(ops);
 	return NULL;
 }
