From 6da1b6260843da455cad8180c18d020679fd4a46 Mon Sep 17 00:00:00 2001
From: Pavel Kubelun <be.dissent@gmail.com>
Date: Sun, 6 Nov 2016 19:07:24 +0300
Subject: [PATCH] ipq806x: add board clocks and rpmcc into DT

Signed-off-by: Pavel Kubelun <be.dissent@gmail.com>
---
 arch/arm/boot/dts/qcom-ipq8064.dtsi | 17 +++++++++++++++++
 1 file changed, 17 insertions(+)

--- a/arch/arm/boot/dts/qcom-ipq8064.dtsi
+++ b/arch/arm/boot/dts/qcom-ipq8064.dtsi
@@ -92,6 +92,18 @@
 	};
 
 	clocks {
+		cxo_board {
+			compatible = "fixed-clock";
+			#clock-cells = <0>;
+			clock-frequency = <25000000>;
+		};
+
+		pxo_board {
+			compatible = "fixed-clock";
+			#clock-cells = <0>;
+			clock-frequency = <25000000>;
+		};
+
 		sleep_clk: sleep_clk {
 			compatible = "fixed-clock";
 			clock-frequency = <32768>;
@@ -175,6 +187,11 @@
 			#address-cells = <1>;
 			#size-cells = <0>;
 
+			rpmcc: clock-controller {
+				compatible	= "qcom,rpmcc-ipq806x", "qcom,rpmcc";
+				#clock-cells = <1>;
+			};
+
 			regulators {
 				compatible = "qcom,rpm-smb208-regulators";
 
