From c97ebdd04db461f38eaa674f29a3f313533221a4 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Tue, 12 Jul 2016 10:35:01 +0100
Subject: [PATCH] BCM270X_DT: Restore lost closing brace.

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/boot/dts/bcm2708-rpi-b.dts | 1 +
 1 file changed, 1 insertion(+)

--- a/arch/arm/boot/dts/bcm2708-rpi-b.dts
+++ b/arch/arm/boot/dts/bcm2708-rpi-b.dts
@@ -36,6 +36,7 @@
 	i2s_pins: i2s {
 		brcm,pins = <28 29 30 31>;
 		brcm,function = <6>; /* alt2 */
+	};
 
 	audio_pins: audio_pins {
 		brcm,pins = <40 45>;
